**DevOps for AIoT - System Requirements Specification (SRS)**

**Automated Gardening System**

Class: DCPE/FT/2A/04

Members:

|  |  |
| --- | --- |
| THEN KAH NYEE | P2223713 |
| ONG SHERN WEN BENJAMIN | P2204484 |
| TAN XING YU JAYDEN | P2204608 |
| CHEN JIAN CONG | P2223528 |
| WONG ZI YANG | P2223768 |

Document version

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No | Updates | Name | Date | Version |
| 1. | Initial version. | Then Kah Nyee | 16 June 2023 | version0.1 |
| 2. | Updates on 1.3 Scope, 2.3 Functional Requirements and 3.1 Static Software Architecture to include more detailed descriptions and revision to python file names. | Then Kah Nyee,  Tan Xing Yu Jayden | 15 July 2023 | version0.2 |
| 3. | Updates on 2.3 Functional Requirements and 3.1 Static Software Infrastructure to include more detailed application layer and changes to REQ-01 to include when the “Start” button is clicked, the text below shall be displayed on the web page.  “System running” | Then Kah Nyee,  Chen Jian Cong,  Tan Xing Yu Jayden | 29 July 2023 | version1.0 |
| 4. | Changes to 2.4 Non-Functional Requirements to replace REQ-21 and REQ-22, Power and Internet Connection to Data Logging as REQ-21 and REQ-22 removed.  Updates on 3.1 Static Software Infrastructure to include newly updated application layer. | Then Kah Nyee,  Chen Jian Cong | 10 August 2023 | version2.0 |

**Table of Contents**

1. Purpose ..............................................................................................................................................

1.1. Intended Audience .....................................................................................................................

1.2. Intended Use ..............................................................................................................................

1.3. Scope ..........................................................................................................................................

1.4. Acronyms and Definitions ..........................................................................................................

1.5. Parameters and Features ...........................................................................................................

2. Overall System Description ................................................................................................................

2.1. Use Case Diagrams .....................................................................................................................

2.2. System Architecture ...................................................................................................................

2.3. Functional Requirements ...........................................................................................................

2.3.1. Start Up and Monitor Parameters .......................................................................................

2.3.2. Dispense Nutrients ..............................................................................................................

2.3.3. Turn On UV Light ..................................................................................................................

2.3.4. Turn On Fan ..........................................................................................................................

2.3.5. Real Time Data Visualisation ................................................................................................

2.4. Non-Functional Requirements ....................................................................................................

2.4.1. Data Logging .........................................................................................................................

3. Software Architecture .........................................................................................................................

3.1. Static Software Architecture ....................................................................................................

1. **Purpose**

**1.1. Intended Audience**

This SRS document describes the System Requirements and Software Design for an Automated Gardening System, and the target audience are System and Software Engineers working on the development of this project.

**1.2. Intended Use**

The SRS defines the overall System Architecture and Requirements as well as the Software Architecture and Design. This document also contains the definition of the System Requirements which shall be used as the input for Manual Test cases and Software Unit Test cases.

**1.3. Scope**

The Automated Gardening System will support the monitoring and control of a hydroponics system for optimal plant growth. The following parameters are monitored continuously:

* pH level of the solution ("Potentiometer" readings)
* Ambient Temperature ("Temperature" readings)
* Relative Humidity ("Humidity" readings)
* Ambient lighting intensity ("LDR" readings)
* EC level ("Moisture sensor" readings)

The automated hydroponics system will be a closed loop system where the simulated EC level ("Moisture sensor" readings) is constantly adjusted to maintain the pre-set optimal level.

* When the simulated EC level is equal to 0, additional nutrient solution will be dispensed into the hydroponics solution by activating a pump based on a servo motor.

The light intensity will also be controlled based on the measured ambient lighting intensity ("LDR" readings) to ensure that plants have optimal lighting at all times.

* When the ambient light intensity level is lower than or equal to 200, a LED (Acting as UV light) will be activated.

Ambient temperature ("Temperature" readings) in the hydroponics system is also maintained at a constant level as much as possible.

* When the ambient temperature is higher than 20, a DC motor (Acting as a fan) is activated to reduce the ambient temperature.

To visualise the data from the different sensors, a dashboard will also be implemented via web page.

**1.4.** **Acronyms and Definitions**

|  |  |
| --- | --- |
| **Acronym** | **Definition** |
| SRS | System Requirements Specification |
| pH | Potential Hydrogen |
| EC | Electrical Conductivity |
| UV | Ultraviolet |
| DHT Sensor | Digital Humidity and Temperature Sensor |
| LDR | Light Dependent Resistor |
| LED | Light Emitting Diode |
| DC | Direct Current |
| IP | Internet Protocol |

**1.5. Parameters and Features**

|  |  |
| --- | --- |
| **Parameters and Features** | **Sensors used to simulate/test Parameters and Features** |
| pH level of the solution | Potentiometer |
| Ambient temperature | DHT sensor |
| Relative humidity | DHT sensor |
| Ambient lighting intensity | LDR |
| EC level | Moisture sensor |
| Nutrient solution pump | Servo motor |
| UV light | LED |
| Fan | DC motor |

1. **Overall System Description**

**2.1. Use Case Diagrams**

A picture containing text, diagram, parallel, receipt

Description automatically generated

**2.2. System Architecture**

A picture containing text, screenshot, fruit

Description automatically generated

**2.3. Functional Requirements**

**2.3.1. Start Up and Monitor Parameters**

|  |  |
| --- | --- |
| **REQ\_ID** | **Requirement** |
| REQ-01 | In the Automated Gardening System web page when the “Start” button is clicked, the text below shall be displayed on the web page.  “System running” |
| REQ-02 | The Automated Gardening System shall be able to continuously simulate the measuring of the pH level of the solution using the potentiometer. The measured readings shall be labelled as "Potentiometer" readings. |
| REQ-03 | The Automated Gardening System shall be able to continuously measure the ambient temperature using the DHT sensor. The measured readings shall be labelled as "Temperature" readings. |
| REQ-04 | The Automated Gardening System shall be able to continuously measure the relative humidity using the DHT sensor. The measured readings shall be labelled as "Humidity" readings. |
| REQ-05 | The Automated Gardening System shall be able to continuously measure the ambient lighting intensity using the LDR. The measured readings shall be labelled as "LDR" readings. |
| REQ-06 | The Automated Gardening System shall be able to continuously simulate the measuring of the EC level of the solution using the moisture sensor. The measured readings shall be labelled as "Moisture sensor" readings. |

**2.3.2. Dispense Nutrients**

The automated hydroponics system maintains the simulated EC level (“Moisture sensor” readings) at the pre-set optimal level by dispensing additional nutrient solution into the hydroponics system. This ensures that the plants always have the optimal nutrient level.

|  |  |
| --- | --- |
| **REQ\_ID** | **Requirement** |
| REQ-07 | From the Moisture sensor, if the "Moisture sensor" reading changes from 1 to 0 then the flowchart defined in Figure 1 would be implemented. |

A diagram of a flowchart

Description automatically generated

REQ-10

REQ-09

REQ-08

Figure 1. Simulated EC Level Optimisation

**2.3.3. Turn On UV Light**

The automated hydroponics system maintains the ambient light intensity at the pre-set optimal level by activating the UV light (LED). This ensures that the plants always have the optimal ambient light intensity.

|  |  |
| --- | --- |
| **REQ\_ID** | **Requirement** |
| REQ-11 | From the LDR, if the "LDR" reading is lower than or equal to 200 the flowchart defined in Figure 2 would be implemented. |

A diagram of a light source

Description automatically generated

REQ-14

REQ-13

REQ-12

Figure 2. Light Intensity Level Optimisation

**2.3.4. Turn On Fan**

The automated hydroponics system maintains the ambient temperature at the pre-set optimal level by turning on the fan (DC motor). This ensures that the plants always have the optimal ambient temperature.

|  |  |
| --- | --- |
| **REQ\_ID** | **Requirement** |
| REQ-15 | From the DHT sensor, if the "Temperature" reading is higher than 20 then the flowchart in Figure 3 would be implemented. |

A diagram of a temperature measurement

Description automatically generated

REQ-18

REQ-17

REQ-16

Figure 3. Temperature Level Optimisation

**2.3.5. Real Time Data Visualisation**

The Automated Gardening System supports “Real Time Data Visualisation” to monitor and visualise the data from the sensors in REQ-02 to REQ-06 on a dashboard via a webpage.

|  |  |
| --- | --- |
| **REQ\_ID** | **Requirement** |
| REQ-19 | The user shall be able to access the IP address of the Automated Gardening System to view a web page. |
| REQ-20 | The web page on the Automated Gardening System shall allow the user to  monitor the following:   * pH level of the solution ("Potentiometer" readings) * Ambient Temperature ("Temperature" readings) * Relative Humidity ("Humidity" readings) * Ambient lighting intensity ("LDR" readings) * EC level ("Moisture sensor" readings) |

**2.4. Non-Functional Requirements**

**2.4.1. Data Logging**

|  |  |
| --- | --- |
| **REQ\_ID** | **Requirement** |
| REQ-21 | The Automated Gardening System shall be able to log data on a daily basis allowing for future references. |

1. **Software Architecture**

**3.1. Static Software Architecture**

The Software Architecture defines the various Software Components that are developed to realise the implementation of the system requirements.

**Application Layer**

A green rectangular box with black text

Description automatically generated A green rectangular box with black text

Description automatically generatedA screenshot of a computer code

Description automatically generated

**Hardware Abstraction Layer (HAL)**

A group of yellow rectangular boxes with black text

Description automatically generated